To Install LeoanrdoSpectrum v2002a (build 44) on Windows 98/NT/2000
****************************************************************************
1. Download the following files:
     LS2002a_win.exe(~31 Mb) - Core executable, libraries, and documentation
     install.pdf  - Installation guide in Adobe Acrobat PDF format
     relnotes.pdf - Enhancements, bug fixes, release overview

2. Install software:
     Double click on LS2002a_win.exe and follow Install Wizard.

3. Install license drivers:
     If running NT using the existing Exemplar dongles, install sentinel
     driver. If using the new GLOBEtrotter dongle, then install dallas
     driver. Required for both Windows NT 4.0 and Windows 95/98.
     
4. To request an evaluation license, visit our web site at:
     http://www.exemplar.com

   Email comments to:
     support@exemplar.com
     sales@exemplar.com

If you have problems extracting downloaded files, try downloading them again.

